#include "BluetoothSerial.h"

#include <Wire.h>

#include <Adafruit\_GFX.h>

#include <Adafruit\_SSD1306.h>

#define SCREEN\_WIDTH 128 // OLED display width, in pixels

#define SCREEN\_HEIGHT 64 // OLED display height, in pixels

// Declaration for an SSD1306 display connected to I2C (SDA, SCL pins)

Adafruit\_SSD1306 display(SCREEN\_WIDTH, SCREEN\_HEIGHT, &Wire, -1);

BluetoothSerial SerialBT;

void setup() {

Serial.begin(115200);

delay(3000);

Serial.println("data");

SerialBT.begin("ESP32test"); //Bluetooth device name

Serial.println("The device has started, now you can pair it with bluetooth!");

if(!display.begin(SSD1306\_SWITCHCAPVCC, 0x3C)) {

Serial.println("SSD1306 allocation failed");

for(;;);

}

delay(1000);

display.clearDisplay();

display.setTextSize(1);

display.setTextColor(WHITE);

display.setCursor(0, 10);

// Display static text

display.println(" ");

display.display();

}

void loop() {

if (Serial.available()) {

SerialBT.write(Serial.read());

}

if (SerialBT.available()) {

String msg=SerialBT.readString();

Serial.println(msg);

String Message(msg);

display.print(Message);

display.display();

delay(100);

}

delay(20);

}